From 60c712da450538836893cfce8618a15240f9eff4 Mon Sep 17 00:00:00 2001
From: Sam Anthony <sam@samanthony.xyz>
Date: Thu, 24 Jul 2025 18:30:53 -0230
Subject: spelling

---
 proposal/proposal.tex | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

(limited to 'proposal/proposal.tex')

diff --git a/proposal/proposal.tex b/proposal/proposal.tex
index 528bd7b..9114a88 100644
--- a/proposal/proposal.tex
+++ b/proposal/proposal.tex
@@ -42,9 +42,9 @@ Testing is the final step.
 Hardware design involves selecting ICs (integrated circuits), creating a circuit schematic, and designing a PCB (printed circuit board).
 Once the board design is finalized, it can be sent for manufacturing.
 
-Two pieces of sofware must be written.
+Two pieces of software must be written.
 The first runs on the microcontroller.
-Essentially, it must communicate with the various peripherals by transforming and transfering data between them.
+Essentially, it must communicate with the various peripherals by transforming and transferring data between them.
 It must fetch frames from the CAN controller and decipher them.
 The CAN data are used to lookup the output value in the ROM.
 Either the PWM peripheral or a DAC is used to send the appropriate signal to the gauge.
-- 
cgit v1.2.3

